Noise Risk Assessment
[DISCLAIMER — DRAFT, FOR SOLICITOR REVIEW] This template is a starting point only. You are responsible for assessing the risks of your own work, and for making sure any document you produce from it is suitable and sufficient for the task, the site and the people involved. It is not health and safety advice.
Use this where people may be exposed to noise at or above the lower exposure action values. Take noise levels from the tool manufacturer’s data or from measurements.
1. Document control
	Company name
	

	Site / location
	

	Assessment reference
	

	Date assessed
	

	Assessed by (name, role)
	

	Review date
	


2. Work activity
	Activity or task
	

	Where it takes place
	

	Who carries it out
	

	Others who could be exposed nearby
	


3. Noise sources
	Tool, plant or process
	Noise level dB(A) (source of figure)
	Time used per person per day
	Who is exposed

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


4. Exposure assessment
Legal values — Control of Noise at Work Regulations 2005, regulation 4:
	
	Daily or weekly exposure
	Peak sound pressure

	Lower exposure action values
	80 dB(A)
	135 dB(C)

	Upper exposure action values
	85 dB(A)
	137 dB(C)

	Exposure limit values (at the ear, taking hearing protection into account)
	87 dB(A)
	140 dB(C)


Your assessment:
	Estimated daily personal exposure (LEP,d)
	

	Highest peak sound pressure
	

	At or above the lower action values? (yes / no)
	

	At or above the upper action values? (yes / no)
	

	Could the exposure limit values be exceeded? (yes / no)
	

	How exposure was estimated (calculator, measurement, manufacturer data)
	


5. Risk rating
Likelihood: 1 Very unlikely · 2 Unlikely · 3 Possible · 4 Likely · 5 Very likely
Severity: 1 Negligible · 2 Minor injury · 3 Injury requiring time off · 4 Major injury · 5 Fatality
Rating bands: 1–4 Low (acceptable, monitor) · 5–12 Medium (reduce where reasonably practicable) · 15–25 High (do not start until reduced)
	
	Likelihood (1–5)
	Severity (1–5)
	Rating (L × S)

	Before controls
	
	
	

	After controls
	
	
	


6. Control measures
	Measure
	Responsible
	Date in place

	Quieter equipment or methods
	
	

	Maintenance of tools and plant to reduce noise
	
	

	Distance, screens or enclosures
	
	

	Limit time spent on noisy tasks
	
	

	Hearing protection zones marked with signs
	
	

	Other
	
	


7. Hearing protection
	Type (ear defenders, plugs)
	

	Rating and suitability for the noise level
	

	Who it is issued to
	

	Training on fitting and use given
	

	How use is checked
	


8. Health surveillance
	Hearing checks needed? (yes / no)
	

	Who provides them
	

	Dates of last and next checks
	


9. Information, instruction and training
	Who
	Training given
	Date

	
	
	

	
	
	

	
	
	


10. Briefing record
I confirm this noise assessment has been explained to me, I understand it, and I will work in line with it.
	Name
	Company
	Signature
	Date
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